Soften Earth and Stone
(Alteration)(Elemental Earth)

Range: 10 yds./level
Components: V, S, M
Duration: Permanent
Casting Time: 5
Area of Effect: 10-ft. square/level
Saving Throw: None
Subtlety: +4	Knockdown: None
Sensory: Moderate visual	Critical: None

	When this spell is cast, all natural, undressed earth or stone in the area of effect is softened. Wet earth becomes thick mud; dry earth becomes loose sand or dirt; and stone becomes soft clay, easily molded or chopped. The priest affects a 10-foot square area to a depth of 1 to 4 feet, depending on the toughness or resilience of the ground at that spot (DM option). Magical or enchanted stone cannot be affected by this spell, nor can dressed or worked stone.
	Creatures attempting to move through an area softened into mud are reduced to a move of 10 feet per round. Any creatures caught within the mud when the spell takes effect must make a saving throw vs. paralyzation or lose the ability to move, attack, or cast spells for 1d2 rounds as they flounder about in the muck. Loose dirt is not as troublesome as mud, and creatures are only reduced to half their normal movement rate, with no chance of being caught for a round or two. However, it is impossible to run, sprint, or charge over either surface.
	Stone softened into clay does not hinder movement, but it does allow characters to cut, shape, or excavate areas they may not have been able to affect before. For example, a party of PCs trying to break out of a cavern might use this spell to soften a wall.
	While soften earth and stone does not affect dressed or worked stone, vertical surfaces such as cliff faces or cavern ceilings can be affected. Usually, this causes a moderate collapse or landslide as the loosened material peels away from the face or roof and falls. A moderate amount of structural damage can be inflicted to man-made structures by softening the ground beneath a wall or tower, causing it to settle. However, most well-built structures will only be damaged by this spell, not destroyed. The material component is a bit of slip (wet clay) from the wheel of a master potter.
